**LEED DATA SHEET**

|  |  |  |
| --- | --- | --- |
| DATE: |  | |
| PROJECT NAME: | |  | |
| PROJECT LOCATION: | |  | |

|  |  |  |
| --- | --- | --- |
| NAME OF PRODUCT: | THERMastic 80 Adhesive | |
| DESCRIPTION: | Hot Applied SEBS Modified Asphalt Elastomeric Roofing Adhesive | |
| PRODUCT/MATERIAL COST: $ | |  |

**SOLAR REFLECTIVITY INDEX (SRI)**

|  |  |
| --- | --- |
| PAVING & SLOPED ROOF >2:12 MUST BE AT LEAST 29: | N/A |
| LOW SLOPED ROOF MATERIALS MUST BE AT LEAST 78: | N/A |

**RECYCLED CONTENT**

|  |  |  |
| --- | --- | --- |
| PRE-CONSUMER: | 0 | % |
| POST CONSUMER: | 0 | % |

**REGIONAL QUALIFICATIONS FOR PRODUCT/MATERIALS:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | DISTANCE FROM PROJECT: |  | MILES |
| LOCATION OF PROCESS: |  | DISTANCE FROM PROJECT: |  | MILES |
| LOCATION OF MANUFACTURE: | Toronto Ontario M4H 1G7 | DISTANCE FROM PROJECT: |  | MILES |

**LOW EMITTING MATERIALS:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| COATING VOC  (GRAMS/L) | SEALANT VOC  (GRAMS/L) | ADHESIVE VOC  (GRAMS/L) | USE OF MATERIAL |  |
|  |  | 0 g/L |  | |

RAPIDLY RENEWABLE MATERIAL:

|  |  |  |
| --- | --- | --- |
| PERCENT RENEWABLE: | 0 | % |
| COST: $ |  |  |

|  |  |
| --- | --- |
| PREPARED BY: |  |

***\*Extraction/Process/Manufacture is defined as the assembly of a final product not including on-site assembly or installation.***

***\*\*Due to several sources of raw materials for this product, specifying the origin of the component materials may not be possible.***